(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1~bpo10+1)
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 310)
    (zones 0)
    (modules 27)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.65 1)
    (pad_drill 0.4)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/pi/Desktop/keyboard-design/rebound/gerbers/"))
  )
  (net 0 "")
  (net 1 D-)
  (net 2 GND)
  (net 3 boot)
  (net 4 "Net-(C1-Pad1)")
  (net 5 "Net-(C2-Pad1)")
  (net 6 +5V)
  (net 7 "Net-(D1-Pad1)")
  (net 8 "Net-(F1-Pad1)")
  (net 9 reset)
  (net 10 MOSI)
  (net 11 SCK)
  (net 12 MISO)
  (net 13 "Net-(LED1-Pad1)")
  (net 14 D+)
  (net 15 "Net-(U1-Pad32)")
  (net 16 "Net-(U1-Pad23)")
  (net 17 "Net-(U1-Pad22)")
  (net 18 "Net-(D2-Pad1)")
  (net 19 PD7)
  (net 20 PD6)
  (net 21 PD5)
  (net 22 PD1)
  (net 23 PD0)
  (net 24 PC7)
  (net 25 PC6)
  (net 26 PC5)
  (net 27 PC4)
  (net 28 PC3)
  (net 29 PC2)
  (net 30 PB4)
  (net 31 PB3)
  (net 32 PB2)
  (net 33 PB1)
  (net 34 PB0)
  (net 35 PA7)
  (net 36 PA6)
  (net 37 PA5)
  (net 38 PA4)
  (net 39 PA3)
  (net 40 PA2)
  (net 41 PA1)
  (net 42 PA0)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net D+)
    (add_net D-)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad32)")
    (add_net PA0)
    (add_net PA1)
    (add_net PA2)
    (add_net PA3)
    (add_net PA4)
    (add_net PA5)
    (add_net PA6)
    (add_net PA7)
    (add_net PB0)
    (add_net PB1)
    (add_net PB2)
    (add_net PB3)
    (add_net PB4)
    (add_net PC2)
    (add_net PC3)
    (add_net PC4)
    (add_net PC5)
    (add_net PC6)
    (add_net PC7)
    (add_net PD0)
    (add_net PD1)
    (add_net PD5)
    (add_net PD6)
    (add_net PD7)
    (add_net SCK)
    (add_net boot)
    (add_net reset)
  )
  (module cftkb:USB_C_GCT_USB4085 (layer F.Cu) (tedit 5ECBC994)
    (at 78.42 66.8 180)
    (fp_text reference USB1 (at -0.017498 1.13737) (layer F.SilkS))
    (fp_text value USB_C_GCT_USB4085 (at 0 0.85) (layer F.Fab))
    (pad S1 thru_hole oval (at 4.325 -1.74 180) (size 0.9 1.7) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
    (pad S1 thru_hole oval (at -4.325 -1.74 180) (size 0.9 1.7) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
    (pad S1 thru_hole oval (at 4.325 -5.12 180) (size 0.9 2.4) (drill oval 0.6 2.1) (layers *.Cu *.Mask))
    (pad S1 thru_hole oval (at -4.325 -5.12 180) (size 0.9 2.4) (drill oval 0.6 2.1) (layers *.Cu *.Mask))
    (pad B1 thru_hole oval (at 2.98 -4.775 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad B4 thru_hole oval (at 2.13 -4.775 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad B5 thru_hole oval (at 1.28 -4.775 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask))
    (pad B6 thru_hole oval (at 0.43 -4.775 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad B7 thru_hole oval (at -0.42 -4.775 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (pad B8 thru_hole oval (at -1.27 -4.775 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask))
    (pad B9 thru_hole oval (at -2.12 -4.775 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 8 "Net-(F1-Pad1)"))
    (pad B12 thru_hole oval (at -2.975 -4.775 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask))
    (pad A12 thru_hole oval (at 2.975 -6.1 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad A9 thru_hole oval (at 2.125 -6.1 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad A8 thru_hole oval (at 1.275 -6.1 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask))
    (pad A7 thru_hole oval (at 0.425 -6.1 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (pad A6 thru_hole oval (at -0.425 -6.1 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad A4 thru_hole oval (at -2.125 -6.1 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 8 "Net-(F1-Pad1)"))
    (pad A1 thru_hole oval (at -2.975 -6.1 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask))
    (pad A5 thru_hole oval (at -1.275 -6.1 180) (size 0.65 1) (drill 0.4) (layers *.Cu *.Mask))
    (model "C:/Users/bryan/Downloads/kicad projects/github repositories/Type-C.pretty/gct-usb4085.step"
      (offset (xyz 0 -2 -0.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "C:/Users/bryan/OneDrive/kicad projects/libraries/Type-C.pretty/USB_C_GCT_USB4085.step"
      (offset (xyz 0 -2 -0.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Keebio-Parts:SinglePad (layer F.Cu) (tedit 5EC9BDF1)
    (at 135.6 69.62)
    (fp_text reference J6 (at 0 -1.778) (layer Dwgs.User) hide)
    (fp_text value PA3 (at 0 1.778) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 39 PA3))
  )
  (module Keebio-Parts:SinglePad (layer F.Cu) (tedit 5EC9BD7D)
    (at 132.79 70.26)
    (fp_text reference J6 (at 0 -1.778) (layer Dwgs.User) hide)
    (fp_text value PA2 (at 0 1.778) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 40 PA2))
  )
  (module locallib:60_Outline-Modded (layer F.Cu) (tedit 5EC99B34)
    (at 202.64 114.6)
    (fp_text reference REF** (at -111.06 -18.08) (layer Dwgs.User) hide)
    (fp_text value 60_Outline (at -107.95 -21.59) (layer F.Fab) hide)
    (fp_line (start 0 -47.3) (end -118.3 -47.3) (layer Edge.Cuts) (width 0.3))
    (fp_arc (start -140.5 -45.3) (end -142.5 -45.3) (angle 90) (layer Edge.Cuts) (width 0.3))
    (fp_line (start -142.5 -34.29) (end -142.5 -45.3) (layer Edge.Cuts) (width 0.3))
    (fp_line (start -129.8 -47.8) (end -118.8 -47.8) (layer Edge.Cuts) (width 0.3))
    (fp_arc (start -130.3 -47.8) (end -129.8 -47.8) (angle 90) (layer Edge.Cuts) (width 0.3))
    (fp_arc (start -118.3 -47.8) (end -118.3 -47.3) (angle 90) (layer Edge.Cuts) (width 0.3))
    (fp_line (start -140.5 -47.3) (end -130.3 -47.3) (layer Edge.Cuts) (width 0.3))
    (pad 1 thru_hole circle (at -115.673654 -17.773654) (size 1 1) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -118.926346 -17.773654) (size 1 1) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -115.673654 -21.026346) (size 1 1) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -118.926346 -21.026346) (size 1 1) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -117.3 -17.1) (size 1 1) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -115 -19.4) (size 1 1) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -119.6 -19.4) (size 1 1) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -117.3 -21.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -117.3 -19.4) (size 7.0013 7.0013) (drill 2.4994) (layers *.Cu *.Mask))
  )
  (module Package_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 5A02E8C5)
    (at 123.305 90.49 90)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U1 (at 7.7 22.325) (layer F.SilkS))
    (fp_text value ATmega32A-PU (at 7.62 50.59 90) (layer F.Fab))
    (fp_text user %R (at 7.62 24.13 90) (layer F.Fab))
    (pad 40 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 PA0))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 PD6))
    (pad 39 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 PA1))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 PD5))
    (pad 38 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 PA2))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 boot))
    (pad 37 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 PA3))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 D-))
    (pad 36 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 PA4))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 D+))
    (pad 35 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 PA5))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 PD1))
    (pad 34 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 PA6))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 PD0))
    (pad 33 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 PA7))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 32 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad32)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad1)"))
    (pad 31 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 30 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 29 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 PC7))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 reset))
    (pad 28 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 PC6))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 SCK))
    (pad 27 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 PC5))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 MISO))
    (pad 26 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 PC4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 MOSI))
    (pad 25 thru_hole oval (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 PC3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 PB4))
    (pad 24 thru_hole oval (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 PC2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 PB3))
    (pad 23 thru_hole oval (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad23)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 PB2))
    (pad 22 thru_hole oval (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad22)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 PB1))
    (pad 21 thru_hole oval (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 PD7))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 PB0))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 66.95 70.04)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 88.87 69.97)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module "" (layer F.Cu) (tedit 5EC96E51)
    (at 76.69 77.64 90)
    (fp_text reference "" (at 0 0 90) (layer F.SilkS))
    (fp_text value "" (at 0 0 90) (layer F.SilkS))
    (pad 25 thru_hole circle (at 0.2286 5.08 90) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(F1-Pad1)"))
    (pad 26 thru_hole circle (at -0.2286 2.54 90) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 27 thru_hole circle (at 0.2286 0 90) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (pad 28 thru_hole circle (at -0.2286 -2.54 90) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
  )
  (module Keebio-Parts:ArduinoProMicro-Mini-USB-ZigZag (layer F.Cu) (tedit 5EC9873C)
    (at 203.7588 82.88528 270)
    (fp_text reference U2 (at 0 1.125 90) (layer F.SilkS) hide)
    (fp_text value ProMicro (at 0 -1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -13.97 10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 42 PA0))
    (pad 2 thru_hole circle (at -11.43 9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 41 PA1))
    (pad 3 thru_hole circle (at -8.89 10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at -6.35 9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -3.81 10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(U1-Pad23)"))
    (pad 6 thru_hole circle (at -1.27 9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(U1-Pad22)"))
    (pad 7 thru_hole circle (at 1.27 10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 38 PA4))
    (pad 8 thru_hole circle (at 3.81 9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 37 PA5))
    (pad 9 thru_hole circle (at 6.35 10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 36 PA6))
    (pad 10 thru_hole circle (at 8.89 9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 35 PA7))
    (pad 11 thru_hole circle (at 11.43 10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 20 PD6))
    (pad 13 thru_hole circle (at 13.97 -9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 14 thru_hole circle (at 11.43 -10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 34 PB0))
    (pad 15 thru_hole circle (at 8.89 -9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 33 PB1))
    (pad 16 thru_hole circle (at 6.35 -10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 32 PB2))
    (pad 17 thru_hole circle (at 3.81 -9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 31 PB3))
    (pad 18 thru_hole circle (at 1.27 -10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 30 PB4))
    (pad 19 thru_hole circle (at -1.27 -9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 23 PD0))
    (pad 20 thru_hole circle (at -3.81 -10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 22 PD1))
    (pad 21 thru_hole circle (at -6.35 -9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 6 +5V))
    (pad 22 thru_hole circle (at -8.89 -10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 23 thru_hole circle (at -11.43 -9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at 13.97 9.8914 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 21 PD5))
    (pad 24 thru_hole circle (at -13.97 -10.3486 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 120.25 83.59 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 9.6 -0.1) (layer F.SilkS))
    (fp_text value 75R (at 3.8 -0.1) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 D-))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-4H_Vertical (layer F.Cu) (tedit 5A1AD3B7)
    (at 152.63 94.59)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 2.44 0) (layer F.SilkS))
    (fp_text value Crystal (at 2.44 3.525) (layer F.Fab))
    (fp_text user %R (at 2.44 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 178.83 82.79)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference RESET1 (at 3.25 -2) (layer F.SilkS))
    (fp_text value RESET (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 reset))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 reset))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 120.25 85.89 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 9.6 0) (layer F.SilkS))
    (fp_text value 75R (at 3.81 -0.1) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 D+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 112.63 88.19)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at -2 0) (layer F.SilkS))
    (fp_text value 1.5k (at 4 0) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 185.89 78.99 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 9.56 0) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 reset))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 112.63 90.49)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at -1.9 0) (layer F.SilkS))
    (fp_text value 1.5K (at 3.8 0.1) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 119.73 77.49 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LED1 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value POWER (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Keebio-Parts:AVR_ICSP_3x2 (layer F.Cu) (tedit 5D3A5A23)
    (at 182.08 73.99 180)
    (descr "Double rangee de contacts 2 x 4 pins")
    (tags CONN)
    (fp_text reference J1 (at 4.195 3.596 180) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 0.120486 0 180) (layer F.SilkS) hide)
    (pad 6 thru_hole circle (at 2.54 -1.27 180) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 2.54 1.27 180) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 reset))
    (pad 4 thru_hole circle (at 0 -1.27 180) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 MOSI))
    (pad 3 thru_hole circle (at 0 1.27 180) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 SCK))
    (pad 2 thru_hole circle (at -2.54 -1.27 180) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 1 thru_hole rect (at -2.54 1.27 180) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 MISO))
    (model pin_array/pins_array_3x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.step
      (offset (xyz 2.5 1.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Keebio-Parts:polyfuse_5.1mm (layer F.Cu) (tedit 5C06210C)
    (at 109.53 70.69)
    (fp_text reference F1 (at 0 -0.025) (layer F.SilkS))
    (fp_text value 500mA (at 0 -1.905) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.55 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 2.55 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/SMKJP.3dshapes/PTC_5.1mm_bend.step
      (offset (xyz 0 0 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P5.08mm_Vertical_AnodeUp (layer F.Cu) (tedit 5AE50CD5)
    (at 105.43 83.79 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 5.08mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 2.4 0 90) (layer F.SilkS))
    (fp_text value 3.6V (at 2.54 2.326371 90) (layer F.Fab))
    (fp_text user A (at 3.58 0.8 90) (layer F.SilkS))
    (fp_text user A (at 3.58 0.8 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.326371 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P5.08mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P5.08mm_Vertical_AnodeUp (layer F.Cu) (tedit 5AE50CD5)
    (at 108.23 83.79 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 5.08mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 2.4 0 90) (layer F.SilkS))
    (fp_text value 3.6V (at 2.54 2.326371 90) (layer F.Fab))
    (fp_text user A (at 3.58 0.8 90) (layer F.SilkS))
    (fp_text user A (at 3.58 0.8 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.326371 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P5.08mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 148.73 72.89 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C5 (at 6.8 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 2.5 0) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 140.43 93.39)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C4 (at -1.9 0 -90) (layer F.SilkS))
    (fp_text value 0.1u (at 2.5 0) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 111.53 78.29 90)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C3 (at 4.047599 0 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0.75 2.9 90) (layer F.SilkS))
    (fp_text user %R (at 0.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 147.83 95.79 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at -2.2 0 180) (layer F.SilkS))
    (fp_text value 22p (at -3.5 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 162.33 95.79 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at -1.8 0 180) (layer F.SilkS))
    (fp_text value 22p (at -3.1 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 178.83 91.39)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BOOT1 (at 3.25 -2) (layer F.SilkS))
    (fp_text value BOOT (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 boot))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 boot))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 78.24 103.07) (end 60.14 80.31) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 195.88 107.48) (end 78.24 103.07) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 215.76 99.27) (end 195.88 107.48) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 215.76 67.3) (end 215.76 99.27) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 202.64 67.3) (end 215.76 67.3) (layer Edge.Cuts) (width 0.3))
  (gr_text GND (at 177.33 75.19 180) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.17 61.98) (xy 220.85 61.18) (xy 218.42 114.75) (xy 60.4 104.25) (xy 58.78 104.25)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.17 60.91) (xy 218.16 63.87) (xy 216 115.02) (xy 59.05 103.98)
      )
    )
  )
)
